Please use this form to provide comments on the Notice of Proposed Amendments for the MUTCD.

**INSTRUCTIONS:**

1. Add your name or organization name where indicted in the footer of this form.
2. Use Table 1 to provide your original comments.
3. Use Table 2 to indicate your agreement with a comment that another commenter has submitted to the docket.
4. Do not adjust formatting of the rows and columns; text will automatically wrap and expand the row height as you type.
5. To add rows to this form, use the “Insert Rows” function, or hover just outside the left edge of the row below which you would like to add a row and click the encircled “+” that appears.
6. If you choose to provide a letter to accompany this comment form, please **print the document as a PDF**; **please do not scan a hard copy**. This will assist FHWA with cataloging your comments.

**TABLE 1. ORIGINAL COMMENTS ON PROPOSED CHANGES.** Please indicate the applicable proposed Section numbers in the far-left column. In the next three columns, please indicate your agreement, disagreement, or whether the column is applicable to your response by placing a, “YES,” “NO,” or “N/A” in the appropriate column of the row. If you agree with a proposed change, then there is no need to fill out the additional columns beyond the first two. However, it can be helpful to explain why you agree with a proposed change based on your objective experience as a roadway operator and/or empirical data. If you disagree in part or in whole, then please provide additional information that FHWA may find helpful.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed  Section Number(s) | Agree with concept and text as proposed | Agree with concept; suggested rewording of text in Comments | Disagree with concept | Comments  *Please include justification for your position based on objective experience and empirical data. If there is a specific statement with which you take exception, please provide the Page and Line numbers from the mark-up version of the proposed MUTCD text.* |
| All |  |  |  | See other file submitted to docket which shows detailed recommended changes to the draft MUTCD text, figures, and tables. |
| 4P.01 | YES | N/A | N/A | NCUTCD agrees with 4P.01 as presented in the NPA. |
| 4P.02 | NO | YES | N/A | NCUTCD recommends revising the second Standard paragraph to state that on 2-lane controlled ramps where the 2 lanes are not controlled separately, only 1 signal face per lane is required in accordance with the 2009 MUTCD and NCUTCD recommendation 14A-STC-01. The NPA changed the requirement to 2 faces per lane based on an Official Interpretation. However, the Official Interpretation itself states that 1 face per lane is sufficient for this condition. With the prevalent use of LED signals, indication failures are rare, and if one face is dark, vehicles only encounter a downstream merge with the other lane, which is not a significant conflict or safety issue. Many ramp signal systems currently operate with one face per controlled lane and no documented safety problems have been reported. NCUTCD also recommends a change in the first Guidance paragraph for consistency with this revision. |
| 4P.03 | YES | N/A | N/A | NCUTCD agrees with 4P.03 as presented in the NPA. |

**TABLE 2. AGREE WITH ANOTHER COMMENTER.** If you agree with another commenter, please indicate the commenter with whom you agree with and note any additional information FHWA may find helpful or any exceptions.

|  |  |  |  |
| --- | --- | --- | --- |
| Docket Comment Number and/or Commenter Name | Agree with commenter’s comments as written | Agree with commenter; with exception(s) | Additional information helpful to FHWA, or exceptions to commenter’s comments |
| (**EXAMPLE**)  FHWA-2020-0001-59 | YES | N/A |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |